{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["插电混动"],"not_rendered":{"images":2},"read":"whole","date_system":"1900"}

{"sheet":"插电混动","index":0,"n_rows":4,"n_cols":12,"rows_kept":4,"merged":[[0,0,0,11],[3,0,3,11]]}
["新疆财经大学后勤公寓服务中心插电混动车辆采购清单及详细参数"]
["序号","品牌及型号","主要参数","颜色","质保","单位","数量","单价（元）","总金额（元）","参考图片","使用部门","使用用途"]
[1,"大众帕萨特C6 1.4T 插电混动","车型Trendline/Fleet  430PHEV 混动商务版 车型号（C6） SVW7143BPV  车型代码(6位) C432ZY 国家目录（工信部公告批次） 342  总长/总宽/总高(mm) 4948/1836/1469；轴距(mm)2871 行李箱容积(L)400 油箱容积(L) 50 整备质量(kg) 1750 发动机排量(L) 1.395 发动机型式 EA211 1.4TSI 110kW+85kW电机，综合功率155kW，400Nm 额定功率/转速(kW/rpm) 110/6000  最大扭矩/转速(Nm/rpm) 250/1750-2000 电机额定功率/转速 (kW/rpm) 55/3090  电机峰值功率/转速 (kW/rpm) 85/6200 电机额定转矩(Nm) 170  电机峰值转矩 (Nm) 330  系统最大功率(kW) 155 系统最大扭矩(Nm) 400  变速箱型式 DQ400e 六速（湿式）双离合变速器  90km/h等速油耗(L/100km) 4.8 (混动) NEDC综合燃料消耗量( L/100km) 1.4  原地起步连续换挡加速时间(s, 0-100km/h) 7.7 混合动力模式最高车速 (km/h) 200 悬架系统 前桥：麦弗逊式独立悬架；后桥：多摆臂式独立悬架 转向系统 电动助力转向系统 制动系统 盘式制动器 排放 国六排放标准 电池能量(kWh) 13 充电效率(KW) 3.6 NEDC纯电动续航里程(km) 63 ","黑色","3年或10万公里","辆",1,{"$nulls":3},"后勤公寓服务中心","乘务车"]
["*备注：供应商须完全响应采购需求清单及详细参数，须上传营业执照、法人身份证复印件、采购报价单（报价单须注明所供产品品牌、型号及报价，报价包含物流和售后人员服务费、安装调试、发票税费等费用）、质保和售后服务承诺函等材料，以上材料均需加盖公章，否则竞价无效。"]